

**Door and tap hardware**

**Performance Statement:**

**Home occupants are able to easily and independently open and close doors and safely use tap hardware.**

**Essential**

No requirements.

**Desirable**

1. Doorways to feature door hardware installed at between 900mm -1100mm above the finished floor. See figure 23.
2. Basins, sinks and tubs to feature lever or capstan style tap hardware with a central spout.

This information was sourced from the national Livable Housing Design Guidelines produced by the National Dialogue on Universal Housing Design.